# TheXCF file format

The XCF-File not only contains mic frequency response data but also contains mic manufacturing, facility and other calibration data. The XCF file is your mic description.

[HEAD];; VERSION;I 13A; CHECK;6H25; [DEV];; MICname;EMX-7150; MICman;iSEMcon GmbH; MICser;4081301; MICpow;Phantom 48V/6,8kOhm; [CAPSULE];; CAPname;MK 204; CAPman;BSWA; CAPtype;Freefield; CAPser;1231623; CAPmV;50; CAPdir;Omnidiectional; | CAPpol;Prepolarized (0V); CAPMICclass;2; [CALIBRATION];; CALfac;iSEMcon GmbH; CALgps;8.591570 49.545144; CALper;Frank; CALdate;16-03-15; CALtemp;22.5; CALhum;37; CALmbar;1013; CALfreq;1000; CALspl;94; CALpow;Phantom 48V/6.8k; MICmV;7.33; | [FRD];; 10.00;-0.83;17.72 11.20;-0.48;18.41 12.50;-0.35;17.23 14.00;-0.20;15.44 …….. 14000.00;1.61;7.10 16000.00;1.64;6.36 18000.00;1.79;5.64 20000.00;1.91;4.65